{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["st_nRF51_1017"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"st_nRF51_1017","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[]}
["Comment","Description","Designator","Footprint","LibRef","Quantity","Value"]
["PAD","","3V3, 5V, 12V, BLE_CLK, BLE_DIO, BLE_RX, BLE_TX, CANH, CANL, GND, P07, PB8, PB9, ST_CLK, ST_DIO, ST_RX, ST_TX","Pad","pad",17]
["ANT","","A1","ANT-F-1-2.4G","ANT",1]
["HDR-1X4","4P接插件","BT_JLINK, BT_UART, ST_JLINK, ST_UART","CONN-TH_530470410","Header 4",4]
["电容","Capacitor","C1, C9, C10, C11, C12, C13, C14, C15, C18, C25, C30, C31","0402","Cap",12,"0.1uF"]
["电容","Capacitor","C2, C7","0402","Cap",2,"20pF"]
["电容","Capacitor","C3, C5, C21, C28, C29","0402","Cap",5,"1uF"]
["电容","Capacitor","C4, C6","0402","Cap",2,"2.2uF"]
["电容","Capacitor","C8","0402","Cap",1,"10uF"]
["电容","Capacitor","C16, C17, C19, C20","0402","Cap",4,"9pF"]
["电容","Capacitor","C22","0402","Cap",1,"22pF"]
["电容","Capacitor","C23","1608[0603]","Cap",1,"10uF"]
["电容","Capacitor","C24","0402","Cap",1,"1pF"]
["电容","Capacitor","C26","1608[0603]","Cap",1,"47nF"]
["电容","Capacitor","C27","0402","Cap",1,"2.2nF"]
["Diode","Default Diode","D1","SOD-123_L2.7-W1.6-LS3.7-RD-1","Diode",1,null,"C8598"]
["Inductor","Inductor","L1","1608[0603]","Inductor",1,"10uH"]
["Inductor","Inductor","L2","0402-A","Inductor",1,"2.4nH"]
["Inductor","Inductor","L3","0402-A","Inductor",1,"5.6nH"]
["Inductor","Inductor","L4","0402-A","Inductor",1,"10nH"]
["LED-0603_R","3.3V电源指示灯","LED_B, LED_G, LED_R","HDR1X2","MHT192IR128CT_1",3]
["Header 2","Header, 2-Pin","P1","HDR1X2","Header 2",1]
["公头","Header, 8-Pin, Dual row","P2","can_pin_16","Header 8X2",1]
["Res2","Resistor","R1, R21","0402","Res2",2,"1K"]
["Res2","Resistor","R2, R3, R4","0402","Res2",3,"10K"]
["Res2","Resistor","R5, R9","6-0805_L","Res2",2,"4.7R"]
["Res2","Resistor","R6, R11","1608[0603]","Res2",2,"51R"]
["Res2","Resistor","R7, R12, R14, R15, R16, R17, R18, R22, R25, R26","0402","Res2",10,"0R"]
["Res2","Resistor","R8","0402","Res2",1,"2K"]
["Res2","Resistor","R10, R13","0402","Res2",2,"1.5K"]
["Res2","Resistor","R19","0402","Res2",1,"0R-NC"]
["Res2","Resistor","R20","0402","Res2",1,"47K"]
["Res2","Resistor","R23, R24","1608[0603]","Res2",2,"0R"]
["nRF51422-QFAC","Multi-protocol Bluetooth Low Energy, ANT and 2.4GHz proprietary system-on-chip","U1","UQFN-48_L6.0-W6.0-P0.40-BL-EP4.6",null,1,"nRF51422-QFAC","C167636"]
["ME6214A50M3G","12v转5v","U2","SOT-23-3_ME6214A50M3G1","ME6214A50M3G",1]
["LP3986-33B3F","5v转3.3","U3","SOT-23-3_ME6214A50M3G1","ME6214A50M3G",1]
["STM32F103RCT6","MCU-stm32f103rct6","U4","LQFP-64_L10.0-W10.0-P0.50-LS12.0-BL","STM32F103RCT6",1,null,"C8323"]
["TJA1050T/CM,118","CAN芯片","U5","SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL","TJA1050T/CM,118",1]
["ME6214C33M5G","","U6","SOT-23-5_ME6214C33M5G","WL2801E33-5/TR",1]
["16MHZ/X322516MLB4SI","","X1","SMD3225-4P","CRYSTAL",1,null,"C13738"]
["8MHZ/10ppm/20pF","Crystal Oscillator","Y1","CRYSTAL-SMD_L5.0-W3.2","XTAL",1,null,"C115962"]
["32.768KHZ","Crystal Oscillator","Y2","OSC-SMD_2012_2P","XTAL",1]