{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["st_nRF51_1017"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"st_nRF51_1017","index":0,"n_rows":32,"n_cols":3,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["Comment","Designator","Footprint"]
["0.1uF","C1, C9, C10, C11, C12, C13, C14, C15, C18, C25, C30, C31","0402"]
["20pF","C2, C7","0402"]
["1uF","C3, C5, C21, C28, C29","0402"]
["2.2uF","C4, C6","0402"]
["10uF","C8","0402"]
["9pF","C16, C17, C19, C20","0402"]
["22pF","C22","0402"]
["10uF","C23","1608[0603]"]
["1pF","C24","0402"]
["47nF","C26","1608[0603]"]
["2.2nF","C27","0402"]
["肖特基二极管","D1","SOD-123_L2.7-W1.6-LS3.7-RD-1"]
["10uH","L1","1608[0603]"]
["2.4nH","L2","0402-A"]
["5.6nH","L3","0402-A"]
["10nH","L4","0402-A"]
["1K","R1, R21","0402"]
["10K","R2, R3, R4","0402"]
["4.7R","R5, R9","6-0805_L"]
["51R","R6, R11","1608[0603]"]
["0R","R7, R12, R14, R15, R16, R17, R18, R22, R25, R26","0402"]
["2K","R8","0402"]
["1.5K","R10, R13","0402"]
["0R-NC","R19","0402"]
["47K","R20","0402"]
["0R","R23, R24","1608[0603]"]
["nRF51422-QFAC","U1","UQFN-48_L6.0-W6.0-P0.40-BL-EP4.6"]
["stm32f103rct6","U4","LQFP-64_L10.0-W10.0-P0.50-LS12.0-BL"]
["TJA1050","U5","SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL"]
["16MHz","X1","SMD3225-4P"]
["8Mhz","Y1","CRYSTAL-SMD_L5.0-W3.2"]